Product program / System Component / Accessory

VP-200VX  BGM

Power amplifier input module for the connection of the power amplifier of the VP-2000 series to the monitoring module of the VX-2000 system with additional mixing input for background music, local feeds, etc. The mixed input can be turned off by a control input, audio signals higher priority, particularly alarming signals and messages without an additional signal transfer. The mixed input should be designed either for symmetrical and stereo audio signals. Transmission of audio signals and control signals for error messages and standby operation.