Product program / Amplifier / System Amplifier

VP-2421

<div>Proof against short power amplifier with 420W power on 50V-, 70V-and 100V-Linien, circuit and open circuit-sure, overheating protection. Cross flow air flow by means of temperature-controlled fan cooling. Connecting the loudspeaker outputs on screw terminal. Slot for different input modules.</div><div>Controllable by the system standby mode with very low power consumption and fast reclosing (&lt; 0.5 seconds).</div><div>&nbsp;</div><div>Operating voltage: 20-40 V =</div><div>Power consumption standby: 33 mA Max&nbsp;</div><div>Rated output power: 420W</div><div>Output voltage: 50V, 70V, 100V</div><div>Frequency response: 40-16000 Hz</div><div>Total harmonic distortion: &lt; 1%</div><div>Signal-to noise ratio: &gt; 80 dB</div><div>Dimensions: 19-inch built-in unit with 2 Unit</div><div>&nbsp;</div><div>Manufacturer: TOA</div><div>Model: VP-2421</div>