Product program / System Component / I/O Units

VX-2000SF

<div>Monitoring basic framework to monitor the power amplifier and automatic switch-over to a spare amplifier as well as monitoring the speaker circuit. 10 Slots for loudspeaker circuit monitoring modules, control input and control output modules. Connection to the System Manager via RJ45 ports, up to 800 meters deductible. Complete monitoring of all audio and control signaling pathways. Simple update system software at the front without Exchange of EPROMs, so that not the whole device to expand.&nbsp;</div><div>LED indicators for power, power supply on and error.</div>