Product program / System Component / Surveillance Modules

VX-200SP-2

Loudspeaker circuit amplifier monitoring module, uninterrupted permanent monitoring short-circuit and interruption via Linienendmodul. Monitoring is carried out also during the transmission of background music and announcements of any kind and does not interrupt them. The amplifier monitoring is also without any interruption. Fault detection for 100 seconds. Switch off the speaker circuit for short circuit. Optional 9-band graphic equalizer can be retrofitted.