Product program / System Component / Surveillance Modules

VX-200SP

Loudspeaker circuit amplifier monitoring module, uninterrupted permanent monitoring short-circuit and interruption by means of rear wiring and ground fault. Monitoring is carried out also during the transmission of background music and announcements of any kind and does not interrupt them. The amplifier monitoring is also without any interruption. Missed Earth detection for 100 seconds. Switch off the speaker circuit for short circuit. Optional 9-band graphic equalizer can be retrofitted.