Product program / System Component / Surveillance Modules

VX-200SZ

Loudspeaker circuit amplifier monitoring module, interruption-free permanent monitoring on short circuits and interruptions by impedance measurement and fault. The impedance measurement is carried out also during the transmission of background music and announcements of any kind and does not interrupt them. The amplifier monitoring is also without any interruption. Fault detection for 100 seconds. Switch off the speaker circuit for short circuit. Optional 9-band graphic equalizer can be retrofitted.