Product program / System Component / I/O Modules

VX-200XI

Input module for microphone and high level signals with control input, adjustable high and low pass filter for Suppression of unwanted noise, phantom power switchable. Transmission of audio signal in programmable output circuits.
&nbsp;
Sensitivity: Microphone: 0.32-7.5 mV
High level: 0,1-2.4 V
High-pass filter 100 Hz: reduction 8 - 14 dB
Low-pass filter 10 kHz: 9 - 15 dB attenuation
Frequency response: 50-20000 Hz
Total harmonic distortion: &lt; 0.5%
Phantom voltage: 15 V
Connector: RJ45