Product program / System Component / Control and Indication Units

VX-3000CT

The control panel shall be an operation panel used with TOA’s VX-3000 System. By connecting the panel to VX-3000's Voice Evacuation Frame via network, the operation such as the activation of general broadcast and the volume control can be performed on its front panel. 
It shall be equipped with 9 function keys and 8 volume controls. A specific function can be assigned to each function key by setting software. Volume control knobs can adjust the volume level of the Voice Evacuation Frame’s audio input or audio output, and which can be set by setting software. Up to 2 units can be connected to a single Voice Evacuation Frame, and a maximum of 80 units can be configured per system.
Power requirements shall be 20 - 33 V DC connected via 4 pin removable terminal block. The unit shall use 1 space unit of a standard EIA component rack space and its dimensions shall be 482 (W) X 44 (H) X 315.2(D) mm (18.98" x 1.73" x 12.41"). Weight shall be 3 kg (6.61lb.) and finished in black surface-treated steel plate front panel, with gray smoke ABS resin volume control section cover.

Manufacturer: TOA Corporation
Model:  VX-3000CT