Product program / System Component / System Manager / Central Unit

VX-3016F

Base frame for 2 amplifier modules with 16 monitored speaker outputs.
The base frame can be configured that one amplifier module operates all 16 speaker outputs or two amplifier modules operate 8 speaker outputs each.
The second amplifier module can alternatively be used as a standby amplifier. 
Up to 4 base frames of this type can be cascaded to increase the number of assignable speaker outputs.
Monitoring is possible by impedance surveillance or by using an end-of-line module.
Settings for impedance deviation to indicate an open or shorted line can be individually set for every output.
4 general balanced audio inputs (microphone/line level) and 2 inputs for up to 8 remote microphones including up to two emergency microphones.
The signals at the general audio inputs can be mixed.
All mandatory indications and controls regarding EN54-16 can be found on the front panel.
Fault indication for every speaker output line.
Redundant network connection (Ethernet) of the base frame with RSTP via two RJ45 ports.
<p class="MsoNormal"/>