Product program / Wireless / Beltpack

WM-5325   G01

UHF Bodypack Transmitter with integrated antenna. Flat casing, switch and power indicator at the top clearly visible and accessible installed. Adjustable microphone sensitivity. Frequency selection out of 64 channels, up to 16 inter modulation free frequencies for simultaneous interference-free transmission of several wireless microphones. Battery condition monitoring with timely reference to necessary battery led on the transmitter and transfer the receiver battery status. Identification signal system to avoid interference when transmitter is switched off in hochfrequenz¬technisch difficult environments. Extremely stable and precise frequency transmitter through quartz stabilized PLL synthesizer. Communication port for PC to change the carrier frequencies adjustable on the transmitter. More than 10 hours of operation with a 1, 5V alkaline AA battery or 13 hours with the optional rechargeable battery WB-2000. Rechargeable in optional charger without battery removal. Carrying case, neck strap and screwdriver to set the frequency in the scope of delivery.