Product program / Wireless / Handheld

WM-D5200    -C7

The digital handheld wireless microphone shall operate in the UHF band between 794 MHz - 832 MHz using the digital true diversity principle to improve reception allowing up to 32 channels of simultaneous broadcast.
The microphone shall utilise a condenser type element with an audio bandwidth of between 100 Hz - 12 kHz and power transmission shall not exceed 50 milliwatts. An internal antenna shall be concealed within the body.
The microphone shall be able to continually operate up to 8 hours on a single AA battery or a dedicated rechargeable battery. There shall be contacts at the base of the unit that will allow easy recharging of the internal rechargeable battery by using a dedicated charger.
The microphone shall have a battery tri-colour status indicator lamp that illuminates from green to orange as battery consumption progresses and then finally red. Battery status will also be transmitted to the receiver.
The microphone shall have an ON/OFF switch that is easily accessible on the exterior of the microphone and by simply twisting and pulling down the handgrip reveals additional functions as follows: bank selection, channel selector, microphone sensitivity selector, encryption setting switch with status indicator, code setting control that prevents interference between channels sharing the same frequency (code setting is effective when the encryption function is not set).
The finished body shall be black coated ABS resin with a steel black head capsule measuring overall ø47 x 239.5 mm (ø1.85" x 9.43") and weighing 220 g (0.49 lb.) (with battery).