Product program / Mixer / Accessory

WP-700-EB

Tender Notice for a Remote Control Switch/Volume Panel

We are seeking a remote control switch and volume panel designed for compatibility with specialized amplifiers. The ideal product should be capable of remote input source selection and volume adjustment when connected to a compatible amplifier. It should also be mountable in a standard 1-gang electrical box of American type.

The required features and specifications include:
- Input Selection: The panel should feature a rotary knob function to select from a minimum of four input lines.
- Volume Control: Capability to adjust the volume level through a rotary knob.
- Connectivity: The panel should offer an RJ-45 connection for linking with the compatible amplifier using a CAT5/5e/6 STP cable.

In terms of connections and compatibility:
- The panel must be compatible with specialized amplifiers, enabling control of up to four such panels.
- The maximum cable length for connection should not exceed 300 feet.

Specifications:
Dimensions: Max. 72 (W) x 128 (H) x 60 (D) mm
Weight: Max. 210g