Product program / Wireless / Receiver / Module

WTU-4800  D01

Wireless tuner module shall be designed to be used in conjunctoin with UHF wireless equipment for vocal or speech reinforcement applications. Its built-in circuit shall minimize the influence of ambient noise.
&nbsp;
Receiving Frequency: 837 - 865 MHz
Receiving System: Double super-heterodyne
Receiving Sensitivity: 80 dB or more, Signal to Noise Raion (20 dbμV input, 40 kHz deviation)
Antenna Input Impedance: 75 ohm
Diversity System: Space diversity
Channel Selectable: 16 channels
Squelch System: Noise Squelch
Squelch Sensitivity: 17 dBµV
Output level: 0 dBV
Total harmonic distortion: 1% or less
Frequency Response: 100 Hz to 12 kHz, -/+ 3 dB
Working temperature range:-10&deg;C to + 50&deg;C (14&deg;F to 122&deg;F)
Dimensions: 60 x 25 x 139 mm (2.36" x 0.98" x 5.47")
Weight: 130 g (0.29 lbs.)
&nbsp;
Manufacturer: TOA
Model: WTU-4800 D01