Product program / Mixer / Modules

WTU-M9800-EBWD1

The tuner module shall have 2 BNC connectors, providing up to 16 channels within the frequency range 794 - 830 MHz. A built-in circuit shall minimize the influence of ambient noise. A contact output terminal shall control external equipment.