Product program / Wireless / Antenna distributor

YW-1024   Y

Signal Distributors (optional) shall be used to expand the number of Infrared Transmitter / Receiver Unit’s which shall not exceed 16 Infrared Transmitter / Receiver Units. The Distributors shall facilitate 1 x 4 configurations. 
Transmission range: 1.6-1000 MHz 
(excluding 50-70 MHz) 
Attenuation: 8.5 dB (+/- 3 dB)
Dimensions (W x H x D): 75 x 122 x 34 mm
Weight: 120 g