Product program / Wireless / Antenna

YW-4500

The remote dipole antenna shall be suitable for use in the UHF frequency range of 550 - 932 MHz. The antenna gain shall be greater than 8 dB with a V. S. W. R. of less than 3. The output impedance shall be 75 ohm with an operating distance of 35 m (115 ft.) maximum using RG-6U cable or 50 m (164 ft.) maximum using RG-11U cable. The antenna power requirement shall be 7- 12 VDC with current consumption of less than 24 mA supplied from the wireless receiver or antenna distributor. The unit shall have a mounting hole pitch of 3.29" (83.5 mm). The operating temperature shall be -10&deg; C to +50&deg; C (+14&deg; F to +122&deg; F). Unit construction shall be AES resin, off-white with dimensions of 105 x 140 x 126 mm (4.13” x 5.51” x 4.96”) and weight of 300 g (0.66 lbs.).