Product program / Mixer / Modules

ZP-001T

Telephone Access Paging to up to eight zones. Uses DTMF dialing to access amplifier and/or line outputs. Dial up to eight output zones in one operation.Analog Extension or Page Port compatible. Page port operation requires contact closure activation and DTMF signal pass-through. RJ-11 Telephone Jack and Removable Terminal Blocks