Product program / Amplifier / Mixer Amplifier

A-1706    UK

Mixer power amplifier with 9 mixing inputs, 
6 balanced microphone inputs with combined jack XLR / phone, 
separately switchable phantom power whereof two inputs can be switched to microphone or high level sensitivity. 
Three recording inputs, of which 2 inputs each with two RCA jacks (stereo) and one input with combined jack XLR / phone jack; 
a recording connector for recording devices with 2 RCA-sockets; 
looping-in of a signal processing device (e.g. equalizers) via RCA jacks; 
Connection for remote control and remote power switch; 
Speaker connections with screw terminals; 
two speaker zones can be switched and a speaker direct output, treble and bass control, sums control; 
Indicators for output level, zone selection, and power; 
desk top design, can be mounted in 19 "cabinet racks with optional brackets MB-25 B, requires 2 units space.