Product program / Amplifier / Mixer Amplifier

A-1724    ER

Mixer power amplifier with 9 mixing inputs, 6 balanced microphone inputs with combined jack XLR / phone, separately switchable phantom power whereof two inputs can be switched to microphone or high level sensitivity. Three recording inputs, of which 2 inputs each with two RCA jacks (stereo) and one input with combined jack XLR / phone jack; a recording connector for recording devices with 2 RCA-sockets; looping-in of a signal processing device (e.g. equalizers) via RCA jacks; Connection for remote control and remote power switch; Speaker connections with screw terminals; two speaker zones can be switched and a speaker direct output, treble and bass control, sums control; Indicators for output level, zone selection, and power; desk top design, can be mounted in 19 "cabinet racks with optional brackets MB-25 B, requires 2 units space.