Product program / Mixer / Modules

AN-9001

Microphone with integrated preamp for uptaking ambient noise levels for ambient noise-driven volume control. Unobtrusive ceiling flush-mounting due to flat white baffle. Rear-mounted removable 3-pin screw terminal. Sensitive electret microphone with half space-shaped polar pattern.