Product program / Mixer / Modules

D-001R

2-channel input module for two stereo sources that are internally mixed to one mono signal each. Adjustable sensitivity range from mic level to line level. High fidelity 24-bit A/D-converter and extremely low distortion. Built-in digital signal processing (DSP) with treble and bass tone control, high and low pass filters and 10 parametric equalizers. Compressor with 5 predefined settings for ease of use. Loudness can be optionally activated.
Connection via two supplied removable 3-pin screw terminals.