Product program / Mixer / Modules

D-001T

2-channel input module for two symmetric Mic / Line sources. Adjustable sensitivity range from microphone level to line level. Phantom power for microphones can be activated. High fidelity through 24-bit A/D-converter and extremely low distortion.&nbsp; Built-in digital signal processing (DSP) with treble and bass tone control, high and low pass filters and 10 parametric equalizers. Compressor with 5 predefined settings for ease of use. Loudness can be optionally activated. Connection via two supplied Plug-in 3-pin connectors.