Product program / Mixer / Modules

D-921F

Input module with two balanced audio inputs. 3-pin XLR jacks for input. Switchable sensitivity and phantom power: on front of the D-901 or via PC software, ground-lift switch.