Product program / Mixer / Modules

D-983

Remote control module with 8 RJ45 jacks for 24 control inputs and 16 floating control outputs. 
Presets, volume adjustment, switching on and off of the inputs or outputs, and selection of the stereo inputs, functions via Windows® software or control elements can be assigned freely to the control inputs.
Simultaneous access on status information at the control outputs to inform the functions of the control inputs as feedback and for interfacing to other systems.