Product program / Mixer / Accessory

M-804EX-EB

<p class="MsoNormal">EXTENSION MODULE 4 PORTS</p>

<p class="MsoNormal">The extension module shall offer 4x additional ports to
extend the number of ports for connecting remote devices.

Port 1: Transmits and receives AES3 digital audio plus control data, connect
to<span>&nbsp; </span>REMOTE MICROPHONE , REMOTE AUDIO
CONTROL PANEL WITH AUDIO OUT , REMOTE AUDIO INPUT OUTPUT PANEL , REMOTE AUDIO
CONTROL PANEL WITH TOUCH DISPLAY , REMOTE AUDIO CONTROL PANEL 

Port 2-4: Transmits and receives control data, connect to<span>&nbsp; </span>REMOTE AUDIO CONTROL PANEL WITH TOUCH DISPLAY
, REMOTE AUDIO CONTROL PANEL </p>

<p class="MsoNormal">The remote audio input output panel must be connected via
Cat5e cable to 8X8 DIGITAL MATRIX MIXER .</p>

<span/>