Product program / System Microphone / Remote Microphone / Stations

N-8000MS  Y

Multifunctional master station with handset and speakerphone with ECHO compensator, LCD display with 16 characters, 2 lines, 8 programmable direct dial keys, connection for headset connection of external speaker, menu functions.
10 Buttons, 4 programmable speed dial buttons, 2 function keys, talk priority button, delete button, call button (for announcement), answer key (for announcement), hold-down button, transfer button (manual call forwarding), redial. 
Function call button for activation control output, call forwarding, Office transfer, time-based call forwarding, busy forwarding, background music.
Connector: RJ-11 connector
&nbsp;
Menu function:
Programming the direct dial keys (follow)
Indicator connected stations at mediation unit
Update function of the operation log (log file), change the IP address, subnet mask, default gateway of the mediation unit with password protection. Setting the system clock, system restart.