Product program / System Microphone / Remote Microphone / Stations

N-8031MS  Y

Single / surface main station with speakerphone with echo cancellation, Wandein-/ build, 4 control inputs for automatic call selection (for example connecting footswitch), optional handset.
10 Buttons, 4 programmable speed dial buttons, 2 function keys, talk priority button, delete button, call button (for announcement), answer key (for announcement), hold-down button, transfer button (manual call forwarding), redial. 
Function call button for activation control output, call forwarding, absence transfer, time-based call forwarding, busy forwarding, background music.