Product program / System Microphone / Remote Microphone / Stations

N-8050DS

Input / building door intercom with speakerphone with echo cancellation, wall-mount, 1 call button, control output (E.g. the door open), dust and water protection: IP54, extended working temperature range