Product program / Système de collaboration audio / NF-CS1

NF-CS1

Window Intercom System Expansion Set

The expansion set for the window intercom system shall consist of one sub-unit, providing a loudspeaker and a microphone, and a distributor for connecting two sub-units to a single audio port.

For the mounting on thick glass windows, an additional self-adhesive magnet shall be included as accessory. Two 3.5 mm mini jack (4P) cables for connecting the distributor to the sub-unit and to another device shall also be included.

Input/output: 3.5 mm mini jack (4P)

Finish: [distributor and sub-unit] ABS resin, white, paint

Dimensions (WxHxD): [Distributor] 36 mm x 30 mm x 15 mm / [sub-unit] 60 mm x 60 mm x 22.5 mm

Weight: [Distributor] 12 g / [sub-unit] 65 g

Manufacturer: TOA

Product: NF-CS1