Product program / System Microphone / Remote Microphone / Stations

RM-200XF

Fire station with easy-to-use hand-held microphone with talk button and 5 programmable buttons, a button with a folding safety cover, expandable to Max 105 keys. Very easy to use with preprogrammed features, including:
- Start and stop warning messages from the text memory in specific sections of the fire 
- Start and stop of evacuation messages from the text store in specific sections of the fire 
- Start and stop of disaster sequences in specific sections of the fire
- Start all-clear messages from the text memory in specific sections of the fire
- Manual announcements in selectable ranges
- Display specific error messages that indicate for example, where (due to damage), no transfer is possible Ready light General error indication, CPU error display, meter. Built-in speaker to listen the amplifier signals and listening with an even tell of programmed pre or post gongs. Adjustable microphone and speaker levels. In the hand-held microphone of built-in beeper to monitor the MIC capsule including the acoustic-electric conversion. Monitoring of control and audio paths, as well as the preamplifier according to EN 60849. 
As an additional safety feature can the CPU at failure of the intercom is switched off and announcements in all areas be discontinued.