Product program / System Microphone / Remote Microphone / Stations

RM-200X   S

System intercom station with Gooseneck microphone and 15 programmable buttons, a button with a folding safety cover, expandable to Max 105 keys. Due to controlled microphone the intercom can be used as emergency intercom. Very easy to use by the programmable functions:
-  Start a disaster sequence through the covered alarm key
-  Manual announcements in selectable ranges
-  Select background music
-  Enable control outputs
-  Listen to the amplifier
-  Change volume
-  Group call
-  Display specific error messages
-  Start of text from the text store
-  Chime activation
When used as a Notfallmkrofon the following additional functions:
-      Start and stop warning messages from the text memory in specific sections of the fire
-      Start and stop of evacuation messages from the text store in specific sections of the fire
-      Start and stop of disaster sequences in specific sections of the fire
-      Start all-clear messages from the text memory in specific sections of the fire
Ready light, General error display and VU-meter. Built-in speaker to listen the amplifier signals and eavesdropping may be programmed first or subsequent gongs. Adjustable microphone and speaker levels.
Monitoring of control and audio paths, as well as the preamplifier according to EN 60849.