Product program / System Microphone / Remote Microphone / Stations

RM-300MF

<div>Fire station with easy-to-use hand-held microphone with talk button. 4 Emergency control buttons, of which a key to trigger the emergency mode with folding safety cover, the other buttons to start warning and evacuation messages and termination of the emergency mode. The intercom is keyboard extensions on expandable up to 65 keys with which other features are possible, including:</div><div>&nbsp;</div><div>- Triggering alerts from the text memory in specific sections of the fire</div><div>- Triggering of evacuation messages from the text memory in specific sections of the fire</div><div>- Manual announcements in selectable ranges&nbsp;</div><div>- standard-compliant acoustic and optical display specific error messages</div><div>&nbsp;</div><div>Firmly integrated failed error communication between station and headquarters, CPU errors and level, ads for readiness. Built-in speaker to the acoustic error message. Adjustable microphone and speaker levels.</div><div>In the hand-held microphone of built-in beeper to monitor the MIC capsule including the acoustic-electric conversion. Monitoring of control and audio paths, as well as the preamplifier according to EN 54-16,&nbsp;</div><div>VDE 0833-4 and VDE 0828-1 (EN 60849).&nbsp;</div><div>As an additional safety feature can failure of the digital control, CPU failure of the intercom is switched off and announcements in all areas be discontinued.</div><div>Wall mount included.</div><div>&nbsp;</div><div>The station is along with the VM-3000 voice alarm system certified by a notified body (notified) according to EN 54-16.</div>