Product program / System Microphone / Remote Microphone / Stations

RM-300X

<div>Elegant remote microphone in desk enclosure and with gooseneck microphone.</div><div>13 free-programmable buttons, talk-button and one button with security cover for emergency functions. Extendable to 85 buttons.</div><div>The remote microphone can be used as emergency microphone due to the monitored microphone capsule.</div><div>Easy operation through pre-programmed functions:</div><div>-<span>	</span>Start of a pre-programmed emergency sequence through the covered alarm button.</div><div>-<span>	</span>Manual paging to selectable areas and group call.</div><div>-<span>	</span>Choosing background music.</div><div>-<span>	</span>Activation of pre-programmed paging’s of any source to any zone.</div><div>-<span>	</span>Indication of specific faults with acknowledge and reset button.</div><div>When used as emergency microphone, additional functions are available:</div><div>-<span>	</span>Start, interrupt, skip and terminate of emergency messages into specific fire areas.</div><div>-<span>	</span>Lamp test.</div><div>Operating-, fault- and level indication.</div><div>Build-in loudspeaker to monitor the pre-programmed start/end chime if applicable.</div><div>Adjustable microphone and loudspeaker level.</div><div>Monitored data and audio lines as well as the pre-amplifier in accordance with EN 60849, EN54-16 and ISO 7240-16.</div>