Product program / Loudspeaker / Box

SR-L05

High-performance subwoofer in bass reflex enclosure, suitable for the 05 series, ideal for mobile application and permanent installation, equipped with a 38 cm (15 ") woofer low-distortion bass reproduction, front panel made of rigid perforated metal mesh with deposited coarsely porous, sound-permeable special foam, connection via 4-pin Speakon connector and screw terminal connection
<p class="MsoNormal">Frequency response: 35 - 1000 Hz

SPL (1W / 1m): 93 dB SPL

Rated Input: 450 W

Impedance: 8 Ohm
<span>Dimensions (W x H x D): 452 x 629 x 502 mm
<span>Weight: 36 kg 
</span></span></p><p class="MsoNormal"><span>Brand: TOA

Type: SR-L05</span></p><p class="MsoNormal"/>