Product program / System Component / Interface

TS-919B1

The Bridge Unit shall be used for connecting a single wired Chairperson/Delegate unit. The Bridge unit shall be directly connected to the dedicated Expansion unit which is connected to the Central unit. Connection between each Bridge unit and the Expansion unit or&nbsp; Chairperson/Delegate unit shall be made with a single CAT-5 LAN cable.

The Bridge Unit shall be the TOA model TS-919B1.