Product program / System Component / Interface

TS-919B4

The Bridge Unit shall be used for connecting up to four wired Chairperson/Delegate units. The Bridge unit shall be directly connected to the dedicated Expansion unit which is connected to the Central unit. Connection between each Bridge unit and the Expansion unit or&nbsp; Chairperson/Delegate unit shall be made with a single CAT-5 LAN cable.

The Bridge Unit shall be the TOA model TS-919B4.