Product program / System Microphone / Conference

TS-923

Gooseneck microphone with red lights ring to display talk released, with two flexible sections. XLR-4-32 connector for connection to the Delegate and Chairperson Units of Infrared Conference systems: TS-820(RC)/TS-920RC.

Sensitivity:-37 dB (1 kHz, 0 dB = 1 V / PA) 
Frequency response: 100 Hz - 13 kHz
Color: black, semi-gloss, paint
Length: 470 mm (1.54 ft)
Weight: 130 g (0.29 lb)
 
The standard microphone unit shall be the TOA model TS-923.