Product program / System Component / I/O Modules

U-01R

The line input module shall be unbalanced, 220k ohms with RCA jack connector.

The line input module shall be TOA model U-01R.