Product program / System Component / I/O Modules

U-03R

<div>The line input module shall be unbalanced, 220k ohms, low/hi-cut filters with stereo summing dual RCA jack connector.</div><div>
</div><div>The line input module shall be TOA model U-03R.</div>