Product program / System Component / I/O Modules

VX-200SI

Control input module, 16 control inputs via optocoupler, each individual input switchable to activation by normally open or normally closed, monitoring the connected control for each input separately programmable. Connection via 4 RJ45 jacks.