Product program / System Component / Surveillance Modules

VX-300SV-EB

End-of-line (EOL) module for 100-volt speaker lines. It schall have a housing with a protection degree of IP65 and a cable gland. It shall provide a ceramic 3-pin screw terminal and a thermal fuse with a cut-off limit of 72°C.