Product program / Wireless / Accessory

WG-D100SK-EB

Synchronisation kit for the tour guide system. An LCD screen shall show the battery level and channel number. Three large buttons shall change the channel or turn off the device. The battery charger bag is needed to synchronize the tour guide system.

The transmitter shall be the TOA model WG-D100T, the receiver shall be the TOA model WG-D100R, the synchronisation kit shall be the TOA model WG-D100SK-EB and the charger shall be the TOA model WG-TC12A.