Product program / Wireless / Handheld

WM-5225   D01

UHF Wireless hand microphone with high sensitivity for voice communications. Stylish enclosure with rubberized surface for secure fit, switch and power indicator on the shaft for intuitively correct operation, rolling stop mechanism prevents the rolling away of the discarded microphone compander system for high system dynamics and low noise,  frequency selection out of 64 channels, up to 16 inter modulation free frequencies for simultaneous interference-free transmission of several wireless microphones, electret microphone capsule with a cardioid pickup pattern and high sensitivity for clear sound, frequency response for good speech intelligibility designed, integrated antenna, Battery condition monitoring with timely indication of necessary battery led display and transmission of battery status to receivers, characteristic signal system to avoid interference when transmitter is switched off in difficult environments. Extremely stable and precise frequency transmitter quartz stabilized PLL synthesizer. Communication port for PC to change the carrier frequencies adjustable on the transmitter. More than 10 hours of operation with a 1, 5V alkaline AA battery or 13 hours with the optional rechargeable battery WB-2000. Rechargeable in optional charger without battery removal. Travel bag, Tripod bracket and screw driver for the frequency setting in the scope of delivery.