Product program / Wireless / Handheld

WM-5270   D04

Professional UHF Wireless hand microphone for vocals and stage, dynamic microphone with cardioid pick-up pattern for extremely high sound pressure levels, frequency response for good reproduction compander system for high system dynamics and low noise, elegant, metal casing for secure grip and noise reduction, no distracting handling the microphone by flat switch in combination with indicator at the end of the shaft, designed, battery condition monitoring with timely indication of necessary battery led on the transmitter and transfer the receiver battery status, Frequency selection out of 64 channels, up to 16 inter modulation free frequencies for simultaneous interference-free transmission of several wireless microphones, built-in antenna, characteristic signal system to avoid interference when transmitter is switched off in difficult environments, extremely stable and precise frequency transmitter PLL synthesizer, maximum input sound pressure level adjustable between 130 dB SPL to 142 dB SPL by a PAD switch, more than 10 hours of operation with a 1, 5V alkaline AA battery, including clamp, carrying bag and micro screwdriver for channel selection.